{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":547,"n_cols":9,"rows_kept":547,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["汕头大学预防性试验项目清单"]
["序号","编号","设备位置","项目名称","数量","单位","综合单价","总价","备注"]
[1,"一","1号开关站"]
[2,null,null,"1、 高压柜（带SF6断路器）",4,"套",null,null,"10KV进、出线柜、母联柜"]
[3,null,null,"1.1 高压柜断路器导电回路电阻测量",4,"组"]
[4,null,null,"1.2 高压柜断路器主回路、辅助回路和控制回路绝缘电阻测量",4,"组"]
[5,null,null,"1.3 高压柜断路器主回路、辅助回路和控制回路交流耐压试验",4,"组"]
[6,null,null,"1.4 高压柜断路器分合闸电磁铁绝缘电阻和直流电阻测量",4,"组"]
[7,null,null,"1.5 高压柜继电保护及二次回路校验",4,"组"]
[8,null,null,"1.6 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",4,"组"]
[9,null,null,"1.7 检查电压抽取（带电显示）装置",4]
[10,null,null,"1.8 五防性能检查",4]
[11,null,null,"小计"]
[12,null,null,"2、高压柜（电压互感器柜）",2,"套"]
[13,null,null,"2.1 高压柜电压互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[14,null,null,"2.2 检查电压抽取（带电显示）装置",2,"组"]
[15,null,null,"2.3 五防性能检查",2,"组"]
[16,null,null,"小计"]
[17,null,null,"3、高压柜（带SF6负荷开关）",2,"套",null,null,"馈电柜"]
[18,null,null,"3.1 高压柜负荷开关相间及相地绝缘电阻测量",16,"组"]
[19,null,null,"3.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",16,"组"]
[20,null,null,"3.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",16,"组"]
[21,null,null,"3.4 检查电压抽取（带电显示）装置",16,"组"]
[22,null,null,"3.5 五防性能检查",16,"组"]
[23,null,null,"小计"]
[24,null,null,"4、FN型户内负荷开关",1,"套"]
[25,null,null,"4.1 负荷开关相间及相地绝缘电阻测量",1,"组"]
[{"$nulls":3},"4.2 交流耐压试验",1,"组"]
[26,null,null,"小计"]
[27,null,null,"5、变压器（油浸式）",1,"套"]
[28,null,null,"5.1 变压器高低压绕组连同套管的绝缘电阻测量",1,"组"]
[29,null,null,"5.2 变压器高低压绕组的直流电阻测量",1,"组"]
[30,null,null,"5.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[31,null,null,"5.4 红外测温",1,"套",null,null,"所有测温点"]
[32,null,null,"小计"]
[33,null,null,"6、10KV母线",2,"段"]
[34,null,null,"6.1 母线绝缘电阻测量",2,"组"]
[35,null,null,"6.2 母线相间及对地交流耐压试验",2,"组"]
[36,null,null,"小计"]
[37,null,null,"7、氧化锌避雷器",2,"套"]
[38,null,null,"7.1 绝缘电阻测量",2,"组"]
[39,null,null,"7.2 氧化锌避雷器1mA电流的电压值U1mA及0.75U1mA的泄露电流",2,"组"]
[40,null,null,"小计"]
[41,null,null,"8、接地装置电阻",2,"套"]
[42,null,null,"8.1 变配电房接地装置的接地电阻测量",2,"组"]
[43,null,null,"8.2 变压器的工作接地电阻测量",2,"组"]
[44,null,null,"小计"]
[45,null,null,"9、10KV电力电缆",2,"根",null,null,"电缆长度：4500米、1000米"]
[46,null,null,"9.1 绝缘电组测量",1,"组"]
[47,null,null,"9.2 交流耐压试验",1,"组"]
[48,null,null,"小计"]
[49,null,null,"合计"]
[50,"二","2号开关站"]
[51,null,null,"1、 高压柜（带SF6断路器）",1,"套",null,null,"10KV进、出线柜、母联柜"]
[52,null,null,"1.1 高压柜断路器导电回路电阻测量",1,"组"]
[53,null,null,"1.2 高压柜断路器主回路、辅助回路和控制回路绝缘电阻测量",1,"组"]
[54,null,null,"1.3 高压柜断路器主回路、辅助回路和控制回路交流耐压试验",1,"组"]
[55,null,null,"1.4 高压柜断路器分合闸电磁铁绝缘电阻和直流电阻测量",1,"组"]
[56,null,null,"1.5 高压柜继电保护及二次回路校验",1,"组"]
[57,null,null,"1.6 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",1,"组"]
[58,null,null,"1.7 检查电压抽取（带电显示）装置",1]
[59,null,null,"1.8 五防性能检查",1]
[60,null,null,"小计"]
[61,null,null,"2、高压柜（电压互感器柜）",1,"套"]
[62,null,null,"2.1 高压柜电压互感器一、二次绕组的绝缘电阻及变比试验",1,"组"]
[63,null,null,"2.2 检查电压抽取（带电显示）装置",1,"组"]
[64,null,null,"2.3 五防性能检查",1,"组"]
[65,null,null,"小计"]
[66,null,null,"3、高压柜（带SF6负荷开关）",8,"套",null,null,"馈电柜"]
[67,null,null,"3.1 高压柜负荷开关相间及相地绝缘电阻测量",8,"组"]
[68,null,null,"3.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",8,"组"]
[69,null,null,"3.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",8,"组"]
[70,null,null,"3.4 检查电压抽取（带电显示）装置",8,"组"]
[71,null,null,"3.5 五防性能检查",8,"组"]
[72,null,null,"小计"]
[73,null,null,"4、FN型户内负荷开关",2,"套"]
[74,null,null,"4.1 负荷开关相间及相地的绝缘电阻测量",2,"组"]
[{"$nulls":3},"4.2 交流耐压试验",2,"组"]
[75,null,null,"小计"]
[76,null,null,"5、变压器（油浸式）",2,"套"]
[77,null,null,"5.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[78,null,null,"5.2 变压器高低压绕组的直流电阻测量",2,"组"]
[79,null,null,"5.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[80,null,null,"5.4 红外测温",2,"套",null,null,"所有测温点"]
[81,null,null,"小计"]
[82,null,null,"6、10KV母线",1,"段"]
[83,null,null,"6.1 母线绝缘电阻测量",1,"组"]
[84,null,null,"6.2 母线相间及对地交流耐压试验",1,"组"]
[85,null,null,"小计"]
[86,null,null,"7、氧化锌避雷器",2,"套"]
[87,null,null,"7.1 绝缘电阻测量",2,"组"]
[88,null,null,"7.2 氧化锌避雷器1mA电流的电压值U1mA及0.75U1mA的泄露电流",2,"组"]
[89,null,null,"小计"]
[90,null,null,"8、接地装置电阻",2,"套"]
[91,null,null,"8.1 变配电房接地装置的接地电阻的测量",2,"组"]
[92,null,null,"8.2 变压器的工作接地电阻测量",2,"组"]
[93,null,null,"小计"]
[94,null,null,"9、10KV电力电缆",1,"根",null,null,"电缆长度：1000米"]
[95,null,null,"9.1 绝缘电组测量",1,"组"]
[96,null,null,"9.2 交流耐压试验",1,"组"]
[97,null,null,"小计"]
[98,null,null,"合计"]
[99,"三","新图书馆"]
[100,null,null,"1、高压柜（带SF6负荷开关）",2,"套",null,null,"进线柜、馈电柜"]
[101,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",2,"组"]
[102,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",2,"组"]
[103,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[104,null,null,"1.4 检查电压抽取（带电显示）装置",2,"组"]
[105,null,null,"1.5 五防性能检查",2,"组"]
[106,null,null,"小计"]
[107,null,null,"2、高压柜（电压互感器柜）",2,"套"]
[108,null,null,"2.1 高压柜电压互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[109,null,null,"2.2 检查电压抽取（带电显示）装置",2,"组"]
[110,null,null,"2.3 五防性能检查",2,"组"]
[111,null,null,"小计"]
[112,null,null,"3、10KV母线",2,"段"]
[113,null,null,"3.1 母线绝缘电阻测量",2,"组"]
[114,null,null,"3.2 母线相间及对地交流耐压试验",2,"组"]
[115,null,null,"小计"]
[116,null,null,"4、变压器（干式）",2,"套"]
[117,null,null,"4.1 变压器高低压绕组的绝缘电阻测量",2,"组"]
[118,null,null,"4.2 变压器高低压绕组的直流电阻测量",2,"组"]
[119,null,null,"4.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[120,null,null,"3.4 红外测温",2,"套"]
[121,null,null,"小计"]
[122,null,null,"5、接地装置电阻",1,"套"]
[123,null,null,"5.1 变配电房接地装置的接地电阻的测量",2,"组"]
[124,null,null,"5.2 变压器的工作接地电阻测量",2,"组"]
[125,null,null,"小计"]
[126,null,null,"6、10KV电力电缆",2,"根",null,null,"电缆长度：650米"]
[127,null,null,"6.1 绝缘电组测量",2,"组"]
[128,null,null,"6.2 交流耐压试验",2,"组"]
[129,null,null,"小计"]
[130,null,null,"合计"]
[131,"四","多学科"]
[132,null,null,"1、高压柜（负荷开关柜）",2,"套",null,null,"进线柜、馈电柜"]
[133,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",2,"组"]
[134,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",2,"组"]
[135,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[136,null,null,"1.4 检查电压抽取（带电显示）装置",2,"组"]
[137,null,null,"1.5 五防性能检查",2,"组"]
[138,null,null,"小计"]
[139,null,null,"2、10KV母线",1,"段"]
[140,null,null,"2.1 母线绝缘电阻测量",1,"组"]
[141,null,null,"2.2 母线相间及对地交流耐压试验",1,"组"]
[142,null,null,"小计"]
[143,null,null,"3、变压器（干式）",1,"套"]
[144,null,null,"3.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[145,null,null,"3.2 变压器高低压绕组的直流电阻测量",1,"组"]
[146,null,null,"3.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[147,null,null,"3.4 红外测温",1,"套"]
[148,null,null,"小计"]
[149,null,null,"4、接地装置电阻",1,"套"]
[150,null,null,"4.1 变配电房接地装置的接地电阻的测量",1,"组"]
[151,null,null,"4.2 变压器的工作接地电阻测量",1,"组"]
[152,null,null,"小计"]
[153,null,null,"5、10KV电力电缆",1,"根",null,null,"电缆长度：480米"]
[154,null,null,"5.1 绝缘电组测量",1,"组"]
[155,null,null,"5.2 交流耐压试验",1,"组"]
[156,null,null,"小计"]
[157,null,null,"合计"]
[158,"五","大礼堂"]
[159,null,null,"1、高压柜（负荷开关柜）",2,"套",null,null,"负荷开关和接地开关为一体化的三工位开关"]
[160,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",2,"组"]
[161,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",2,"组"]
[162,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[163,null,null,"1.4 检查电压抽取（带电显示）装置",2,"组"]
[164,null,null,"1.5 五防性能检查",2,"组"]
[165,null,null,"小计"]
[166,null,null,"2、变压器（干式）",1,"套"]
[167,null,null,"2.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[168,null,null,"2.2 变压器高低压绕组的直流电阻测量",1,"组"]
[169,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[170,null,null,"2.4 红外测温",1,"套"]
[171,null,null,"小计"]
[172,null,null,"3、接地装置电阻",1,"套"]
[173,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[174,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[175,null,null,"小计"]
[176,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：440米"]
[177,null,null,"4.1 绝缘电组测量",1,"组"]
[178,null,null,"4.2 交流耐压试验",1,"组"]
[179,null,null,"小计"]
[180,null,null,"合计"]
[181,"六","风洞实验室"]
[182,null,null,"1、FN型户内负荷开关",1,"套"]
[183,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[184,null,null,"小计"]
[185,null,null,"2、变压器（干式）",1,"套",null,null,"整流变压器"]
[186,null,null,"2.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[187,null,null,"2.2 变压器高低压绕组的直流电阻测量",1,"组"]
[188,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[189,null,null,"2.4 红外测温",1,"套"]
[190,null,null,"小计"]
[191,null,null,"3、接地装置电阻",1,"套"]
[192,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[193,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[194,null,null,"小计"]
[195,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：420米"]
[196,null,null,"4.1 绝缘电组测量",1,"组"]
[197,null,null,"4.2 交流耐压试验",1,"组"]
[198,null,null,"小计"]
[199,null,null,"合计"]
[200,"七","科技楼"]
[201,null,null,"1、FN型户内负荷开关",1,"套"]
[202,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[{"$nulls":3},"1.2 交流耐压试验",1,"组"]
[203,null,null,"小计"]
[204,null,null,"2、变压器（油浸式）",2,"套",null,null,"有载调压变压器"]
[205,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[206,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[207,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[208,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[209,null,null,"小计"]
[210,null,null,"3、接地装置电阻",1,"套"]
[211,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[212,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[213,null,null,"小计"]
[214,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：50米"]
[215,null,null,"4.1 绝缘电组测量",1,"组"]
[216,null,null,"4.2 交流耐压试验",1,"组"]
[217,null,null,"小计"]
[218,null,null,"合计"]
[219,"八","工科楼"]
[220,null,null,"1、FN型户内负荷开关",1,"套"]
[221,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[222,null,null,"1.2 交流耐压试验",1,"组"]
[223,null,null,"小计"]
[224,null,null,"2、变压器（油浸式）",2,"套"]
[225,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[226,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[227,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[228,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[229,null,null,"小计"]
[230,null,null,"3、接地装置电阻",1,"套"]
[231,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[232,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[233,null,null,"小计"]
[234,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：140米"]
[235,null,null,"4.1 绝缘电组测量",1,"组"]
[236,null,null,"4.2 交流耐压试验",1,"组"]
[237,null,null,"小计"]
[238,null,null,"合计"]
[259,"九","教授楼"]
[260,null,null,"1、高压柜（负荷开关柜）",4,"套",null,null,"进线柜、馈电柜"]
[261,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",4,"组"]
[262,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",4,"组"]
[263,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",4,"组"]
[264,null,null,"1.4 检查电压抽取（带电显示）装置",4,"组"]
[265,null,null,"1.5 五防性能检查",4,"组"]
[266,null,null,"小计"]
[267,null,null,"2、10KV母线",1,"段"]
[268,null,null,"2.1 母线绝缘电阻测量",1,"组"]
[269,null,null,"2.2 母线相间及对地交流耐压试验",1,"组"]
[270,null,null,"小计"]
[271,null,null,"3、变压器（干式）",1,"套"]
[272,null,null,"3.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[273,null,null,"3.2 变压器高低压绕组的直流电阻测量",1,"组"]
[274,null,null,"3.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[275,null,null,"3.4 红外测温",1,"套"]
[276,null,null,"小计"]
[277,null,null,"4、接地装置电阻",1,"套"]
[278,null,null,"4.1 变配电房接地装置的接地电阻的测量",1,"组"]
[279,null,null,"4.2 变压器的工作接地电阻测量",1,"组"]
[280,null,null,"小计"]
[281,null,null,"5、10KV电力电缆",1,"根",null,null,"电缆长度：450米"]
[282,null,null,"5.1 绝缘电组测量",1,"组"]
[283,null,null,"5.2 交流耐压试验",1,"组"]
[284,null,null,"小计"]
[285,null,null,"合计"]
[286,"十","学术交流中心"]
[287,null,null,"1、FN型户内负荷开关",1,"套"]
[288,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[289,null,null,"1.2 交流耐压试验",1,"组"]
[290,null,null,"小计"]
[291,null,null,"2、变压器（油浸式）",2,"套"]
[292,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[293,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[294,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[295,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[296,null,null,"小计"]
[297,null,null,"3、接地装置电阻",1,"套"]
[298,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[299,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[300,null,null,"小计"]
[301,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：440米"]
[302,null,null,"4.1 绝缘电组测量",1,"组"]
[303,null,null,"4.2 交流耐压试验",1,"组"]
[304,null,null,"小计"]
[305,null,null,"合计"]
[306,"十一","理科楼"]
[307,null,null,"1、FN型户内负荷开关",1,"套"]
[308,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[309,null,null,"1.2 交流耐压试验",1,"组"]
[310,null,null,"小计"]
[311,null,null,"2、变压器（油浸式）",2,"套"]
[312,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[313,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[314,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[315,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[316,null,null,"小计"]
[317,null,null,"3、接地装置电阻",1,"套"]
[318,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[319,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[320,null,null,"小计"]
[321,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：210米"]
[322,null,null,"4.1 绝缘电组测量",1,"组"]
[323,null,null,"4.2 交流耐压试验",1,"组"]
[324,null,null,"小计"]
[325,null,null,"合计"]
[326,"十二","学生宿舍"]
[327,null,null,"1、高压柜（负荷开关柜）",2,"套",null,null,"进线柜、馈电柜"]
[328,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",2,"组"]
[329,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",2,"组"]
[330,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[331,null,null,"1.4 检查电压抽取（带电显示）装置",2,"组"]
[332,null,null,"1.5 五防性能检查",2,"组"]
[333,null,null,"小计"]
[334,null,null,"2、10KV母线",1,"段"]
[335,null,null,"2.1 母线绝缘电阻测量",1,"组"]
[336,null,null,"2.2 母线相间及对地交流耐压试验",1,"组"]
[337,null,null,"小计"]
[338,null,null,"3、变压器（干式）",1,"套"]
[339,null,null,"3.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[340,null,null,"3.2 变压器高低压绕组的直流电阻测量",1,"组"]
[341,null,null,"3.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[342,null,null,"3.4 红外测温",1,"套"]
[343,null,null,"小计"]
[344,null,null,"4、接地装置电阻",1,"套"]
[345,null,null,"4.1 变配电房接地装置的接地电阻的测量",1,"组"]
[346,null,null,"4.2 变压器的工作接地电阻测量",1,"组"]
[347,null,null,"小计"]
[348,null,null,"5、10KV电力电缆",1,"根",null,null,"电缆长度：203米"]
[349,null,null,"5.1 绝缘电组测量",1,"组"]
[350,null,null,"5.2 交流耐压试验",1,"组"]
[351,null,null,"小计"]
[352,null,null,"合计"]
[353,"十三","教工宿舍"]
[354,null,null,"1、高压柜（负荷开关柜）",2,"套",null,null,"进线柜、馈电柜"]
[355,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",2,"组"]
[356,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",2,"组"]
[357,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[358,null,null,"1.4 检查电压抽取（带电显示）装置",2,"组"]
[359,null,null,"1.5 五防性能检查",2,"组"]
[360,null,null,"小计"]
[361,null,null,"2、10KV母线",1,"段"]
[362,null,null,"2.1 母线绝缘电阻测量",1,"组"]
[363,null,null,"2.2 母线相间及对地交流耐压试验",1,"组"]
[364,null,null,"小计"]
[365,null,null,"3、变压器（干式）",1,"套"]
[366,null,null,"3.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[367,null,null,"3.2 变压器高低压绕组的直流电阻测量",1,"组"]
[368,null,null,"3.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[369,null,null,"3.4 红外测温",1,"套"]
[370,null,null,"小计"]
[371,null,null,"4、接地装置电阻",1,"套"]
[372,null,null,"4.1 变配电房接地装置的接地电阻的测量",1,"组"]
[373,null,null,"4.2 变压器的工作接地电阻测量",1,"组"]
[374,null,null,"小计"]
[375,null,null,"5、10KV电力电缆",1,"根",null,null,"电缆长度：640米"]
[376,null,null,"5.1 绝缘电组测量",1,"组"]
[377,null,null,"5.2 交流耐压试验",1,"组"]
[378,null,null,"小计"]
[379,null,null,"合计"]
[380,"十四","西区水泵房"]
[381,null,null,"1、高压柜（负荷开关柜）",4,"套",null,null,"进线柜、馈电柜"]
[382,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",4,"组"]
[383,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",4,"组"]
[384,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",4,"组"]
[385,null,null,"1.4 检查电压抽取（带电显示）装置",4,"组"]
[386,null,null,"1.5 五防性能检查",4,"组"]
[387,null,null,"小计"]
[388,null,null,"2、10KV母线",1,"段"]
[389,null,null,"2.1 母线绝缘电阻测量",1,"组"]
[390,null,null,"2.2 母线相间及对地交流耐压试验",1,"组"]
[391,null,null,"小计"]
[392,null,null,"3、变压器（干式）",1,"套"]
[393,null,null,"3.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[394,null,null,"3.2 变压器高低压绕组的直流电阻测量",1,"组"]
[395,null,null,"3.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[396,null,null,"3.4 红外测温",1,"套"]
[397,null,null,"小计"]
[398,null,null,"4、接地装置电阻",1,"套"]
[399,null,null,"4.1 变配电房接地装置的接地电阻的测量",1,"组"]
[400,null,null,"4.2 变压器的工作接地电阻测量",1,"组"]
[401,null,null,"小计"]
[402,null,null,"5、10KV电力电缆",1,"根",null,null,"电缆长度：1250米"]
[403,null,null,"5.1 绝缘电组测量",1,"组"]
[404,null,null,"5.2 交流耐压试验",1,"组"]
[405,null,null,"小计"]
[406,null,null,"合计"]
[407,"十五","医科楼"]
[408,null,null,"1、高压柜（负荷开关柜）",1,"套",null,null,"负荷开关和接地开关为一体化的三工位开关"]
[409,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",1,"组"]
[410,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",1,"组"]
[411,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",1,"组"]
[412,null,null,"1.4 检查电压抽取（带电显示）装置",1,"组"]
[413,null,null,"1.5 五防性能检查",1,"组"]
[414,null,null,"小计"]
[415,null,null,"2、变压器（干式）",1,"套"]
[416,null,null,"2.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[417,null,null,"2.2 变压器高低压绕组的直流电阻测量",1,"组"]
[418,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[419,null,null,"2.4 红外测温",1,"套"]
[420,null,null,"小计"]
[421,null,null,"3、接地装置电阻",1,"套"]
[422,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[423,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[424,null,null,"小计"]
[425,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：430米"]
[426,null,null,"4.1 绝缘电组测量",1,"组"]
[427,null,null,"4.2 交流耐压试验",1,"组"]
[428,null,null,"小计"]
[429,null,null,"合计"]
[430,"十六","网络中心"]
[431,null,null,"1、高压柜（负荷开关柜）",1,"套",null,null,"负荷开关和接地开关为一体化的三工位开关"]
[432,null,null,"1.1 高压柜负荷开关相间及相地绝缘电阻测量",1,"组"]
[433,null,null,"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",1,"组"]
[434,null,null,"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",1,"组"]
[435,null,null,"1.4 检查电压抽取（带电显示）装置",1,"组"]
[436,null,null,"1.5 五防性能检查",1,"组"]
[437,null,null,"小计"]
[438,null,null,"2、变压器（干式）",1,"套"]
[439,null,null,"2.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[440,null,null,"2.2 变压器高低压绕组的直流电阻测量",1,"组"]
[441,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[442,null,null,"2.4 红外测温",1,"套"]
[443,null,null,"小计"]
[444,null,null,"3、接地装置电阻",1,"套"]
[445,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[446,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[447,null,null,"小计"]
[448,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：112米"]
[449,null,null,"4.1 绝缘电组测量",1,"组"]
[450,null,null,"4.2 交流耐压试验",1,"组"]
[451,null,null,"小计"]
[452,null,null,"合计"]
[453,"十七","体育馆"]
[454,null,null,"1、FN型户内负荷开关",1,"套"]
[455,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[456,null,null,"1.2 交流耐压试验",1,"组"]
[457,null,null,"小计"]
[458,null,null,"2、变压器（干式）",1,"套"]
[459,null,null,"2.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[460,null,null,"2.2 变压器高低压绕组的直流电阻测量",1,"组"]
[461,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[462,null,null,"2.4 红外测温",1,"套",null,null,"所有测温点"]
[463,null,null,"小计"]
[464,null,null,"3、接地装置电阻",1,"套"]
[465,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[466,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[467,null,null,"小计"]
[468,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：100米"]
[469,null,null,"4.1 绝缘电组测量",1,"组"]
[470,null,null,"4.2 交流耐压试验",1,"组"]
[471,null,null,"小计"]
[472,null,null,"合计"]
[473,"十八","文科楼"]
[474,null,null,"1、FN型户内负荷开关",1,"套"]
[475,null,null,"1.1 负荷开关相间及相地的绝缘电阻测量",1,"组"]
[476,null,null,"1.2 交流耐压试验",1,"组"]
[477,null,null,"小计"]
[478,null,null,"2、变压器（油浸式）",2,"套"]
[479,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[480,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[481,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[482,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[483,null,null,"小计"]
[484,null,null,"3、接地装置电阻",1,"套"]
[485,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[486,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[487,null,null,"小计"]
[488,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：100米"]
[489,null,null,"4.1 绝缘电组测量",1,"组"]
[490,null,null,"4.2 交流耐压试验",1,"组"]
[491,null,null,"小计"]
[492,null,null,"合计"]
[493,"十九","龙泉园"]
[494,null,null,"1、户外交流高压跌落式熔断器",1,"套"]
[495,null,null,"1.1 高压跌落式熔断器相间及相地的绝缘电阻测量",1,"组"]
[496,null,null,"1.2 交流耐压试验",1,"组"]
[497,null,null,"小计"]
[498,null,null,"2、变压器（油浸式）",2,"套"]
[499,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[500,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[501,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[502,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[503,null,null,"小计"]
[504,null,null,"3、接地装置电阻",1,"套"]
[505,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[506,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[507,null,null,"小计"]
[508,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：100米"]
[509,null,null,"4.1 绝缘电组测量",1,"组"]
[510,null,null,"4.2 交流耐压试验",1,"组"]
[511,null,null,"小计"]
[512,null,null,"合计"]
[513,"二十","成教学院"]
[514,null,null,"1、户外交流高压跌落式熔断器",1,"套"]
[515,null,null,"1.1 高压跌落式熔断器相间及相地的绝缘电阻测量",1,"组"]
[516,null,null,"1.2 交流耐压试验",1,"组"]
[517,null,null,"小计"]
[518,null,null,"2、变压器（油浸式）",2,"套"]
[519,null,null,"2.1 变压器高低压绕组连同套管的绝缘电阻测量",2,"组"]
[520,null,null,"2.2 变压器高低压绕组的直流电阻测量",2,"组"]
[521,null,null,"2.3 变压器测温装置及二次回路的绝缘电阻测量",2,"组"]
[522,null,null,"2.4 红外测温",2,"套",null,null,"所有测温点"]
[523,null,null,"小计"]
[524,null,null,"3、接地装置电阻",1,"套"]
[525,null,null,"3.1 变配电房接地装置的接地电阻的测量",1,"组"]
[526,null,null,"3.2 变压器的工作接地电阻测量",1,"组"]
[527,null,null,"小计"]
[528,null,null,"4、10KV电力电缆",1,"根",null,null,"电缆长度：500米"]
[529,null,null,"4.1 绝缘电组测量",1,"组"]
[530,null,null,"4.2 交流耐压试验",1,"组"]
[531,null,null,"小计"]
[532,null,null,"合计"]
[null,"二十一","新行政中心"]
[{"$nulls":3},"1、高压柜（负荷开关柜）",2,"套",null,null,"进线柜、PT柜(计量柜)、馈电柜"]
[{"$nulls":3},"1.1 高压柜负荷开关相间及相地绝缘电阻测量",2,"组"]
[{"$nulls":3},"1.2 高压柜负荷开关主回路、辅助回路和控制回路交流耐压试验",2,"组"]
[{"$nulls":3},"1.3 高压柜电流互感器一、二次绕组的绝缘电阻及变比试验",2,"组"]
[{"$nulls":3},"1.4 检查电压抽取（带电显示）装置",2,"组"]
[{"$nulls":3},"1.5 五防性能检查",2,"组"]
[{"$nulls":3},"小计"]
[{"$nulls":3},"2、10KV母线",1,"段"]
[{"$nulls":3},"2.1 母线绝缘电阻测量",1,"组"]
[{"$nulls":3},"2.2 母线相间及对地交流耐压试验",1,"组"]
[{"$nulls":3},"小计"]
[{"$nulls":3},"3、变压器（干式）",1,"套"]
[{"$nulls":3},"3.1 变压器高低压绕组的绝缘电阻测量",1,"组"]
[{"$nulls":3},"3.2 变压器高低压绕组的直流电阻测量",1,"组"]
[{"$nulls":3},"3.3 变压器测温装置及二次回路的绝缘电阻测量",1,"组"]
[{"$nulls":3},"3.4 红外测温",1,"套"]
[{"$nulls":3},"小计"]
[533,"二十二","安全工具"]
[534,null,null,"1、高压交流验电器",1,"套"]
[535,null,null,"1.1 交流耐压",1,"组"]
[536,null,null,"2、高压交流验电器绝缘棒",2,"套"]
[537,null,null,"2.1 交流耐压",2,"组"]
[538,null,null,"3、绝缘靴",2,"套"]
[539,null,null,"3.1 交流耐压",2,"组"]
[540,null,null,"4、绝缘手套",2,"套"]
[541,null,null,"4.1 交流耐压",2,"组"]
[{"$nulls":3},"小计"]
[{"$nulls":3},"合计"]
[null,null,"总计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}